

iCUBE-iCON Release Notes

* **Latest Release: iCUBE 0x0106, iCON 0x0206**
* **Release Date:** Oct 06, 2023

Revision History

|  |  |  |  |
| --- | --- | --- | --- |
| Version | Date | Description | Authors |
| 0x106,  0x206 | Oct 06, 2023 | Prevent solar charging timeout is changed to 10 seconds from 5 seconds. FT exit if temperature exceeds a threshold value | Vineeth |
| 0x105,  0x205 | Aug 31, 2023 | Issue of not calling log api is fixed | Vineeth |
| 0x0104,  0x0204 | Aug 05, 2023 | Improved device configuration, Fixed data loss with wrong EEPROM read, Fixed PAC ERROR reset issue | Vineeth |
| 0x0103, 0x0203 | June 03, 2023 | Fix for ‘Device not configured’ issue, Restart the device if Wi-Fi fails to connect at the starting, blue led 10 second blink introduced for test connectivity,  WiFi disconnects after sending data to server. | Vineeth |
| 0x0102,  0x0202 | May 17, 2023 | Fix to reduce data latency and data loss issues, RED LED 5 second blink when mains failure detected, is removed, SSID name will have version string | Vineeth |
| 0x0101,  0x0200 | May 12,2023 | Fix for issue of using Configuration tool and mobile app, Fix for connectivity test issue | Vineeth |
| 0x0100,  0x0200 | May 04 ,2023 | Initial stable release | Vineeth |

Table of Contents

[Revision History 2](#__RefHeading___Toc9630_1894761172)

[V- iCUBE 0x0106, iCON 0x0206 5](#__RefHeading___Toc4893_134704998411111)

[Enhancements/Fixes to Existing Features 5](#__RefHeading___Toc335_3054807761111)

[Changed prevent solar charging timeout 5](#__RefHeading___Toc456_9599016811)

[FT exit if temperature reaches a threshold 5](#__RefHeading___Toc456_95990168111)

[V- iCUBE 0x0105, iCON 0x0205 5](#__RefHeading___Toc4893_13470499841111)

[Enhancements/Fixes to Existing Features 5](#__RefHeading___Toc335_305480776111)

[Issue of not calling log api is fixed 5](#__RefHeading___Toc456_959901681)

[V- iCUBE 0x0104, iCON 0x0204 5](#__RefHeading___Toc4893_1347049984111)

[Enhancements/Fixes to Existing Features 5](#__RefHeading___Toc335_30548077611)

[Improved device configuration using mobile app 5](#__RefHeading___Toc456_95990168)

[Fixed data loss issue 5](#__RefHeading___Toc454_95990168)

[Device multiple reset due to PAC ERROR fixed 5](#__RefHeading___Toc452_95990168)

[V- iCUBE 0x0103, iCON 0x0203 5](#__RefHeading___Toc4893_134704998411)

[Enhancements/Fixes to Existing Features 5](#__RefHeading___Toc335_3054807761)

[Restart the device if fails to connect the Wi-Fi at startup 5](#__RefHeading___Toc337_3054807761)

[Fix for the ‘Device not configured’ issue. 6](#__RefHeading___Toc339_3054807761)

[Blue LED 10 second stable state 6](#__RefHeading___Toc341_3054807761)

[WiFi disconnects after sending data to server 6](#__RefHeading___Toc341_30548077611)

[V- iCUBE 0x0102, iCON 0x0202 6](#__RefHeading___Toc4893_13470499841)

[Enhancements/Fixes to Existing Features 6](#__RefHeading___Toc4794_170861885912)

[Chance for data latency/data loss due to the code loopholes are fixed 6](#__RefHeading___Toc243_2317239721)

[Frequent connection/disconnection of Wi-Fi is avoided 6](#__RefHeading___Toc245_2317239721)

[RED LED in 5 second blink when mains failure is detected, removed. 6](#__RefHeading___Toc247_2317239721)

[SSID Name exposed by the device will have firmware version string at the end 6](#__RefHeading___Toc1205_2317239721)

[V- iCUBE 0x0101, iCON 0x0201 6](#__RefHeading___Toc4893_1347049984)

[Enhancements/Fixes to Existing Features 6](#__RefHeading___Toc4794_17086188591)

[Issue in using Configuration tool and mobile app is fixed 6](#__RefHeading___Toc5878_434370227)

[‘Connectivity test’ issue is fixed 6](#__RefHeading___Toc214_3688195712)

[Known issues 6](#__RefHeading___Toc211_1165673383)

[When tested mobile application using a mobile phone Xiaomi MiA1 android version 9 , socket connection to the device is not happening when mobile data is ON. 7](#__RefHeading___Toc213_1165673383)

[V- iCUBE 0x0100, iCON 0x0200 7](#__RefHeading___Toc5885_434370227)

[Enhancements/Fixes to Existing Features 7](#__RefHeading___Toc4794_170861885911)

[First stable release 7](#__RefHeading___Toc5878_4343702271)

# V- iCUBE 0x0106, iCON 0x0206

## Enhancements/Fixes to Existing Features

### Changed prevent solar charging timeout

Prevent solar charging timeout is changed to 10 seconds from 5 seconds

### FT exit if temperature reaches a threshold

When device is in Force Trip state, if temperature (Temperature1) reaches a threshold level, device exit from FT and will enter into FT after 30 minutes only.

# V- iCUBE 0x0105, iCON 0x0205

## Enhancements/Fixes to Existing Features

### Issue of not calling log api is fixed

Some devices at sometimes was not sending logs to server but other api calls were ok. This has been fixed.

# V- iCUBE 0x0104, iCON 0x0204

## Enhancements/Fixes to Existing Features

### Improved device configuration using mobile app

Sometimes when doing device configuration multiple times, it is seen that device is not able to serve the mobile app. Fix for this issue is added.

### **Fixed data loss issue**

When data is read from EEPROM, and reaches at the end region of data, device was reading some region outside the data boundary and that data will be of invalid and server rejects that value and no graph will be drawn. Hence data loss issue for a small block is seen. Fix for this is added.

### Device multiple reset due to PAC ERROR fixed

When if one pac sensor read was failed, it was setting as PAC ERROR and device exit from force trip. This is changed in such a way that PAC ERROR is set if pac sensor reading fails for 3 times continuously.

# V- iCUBE 0x0103, iCON 0x0203

## Enhancements/Fixes to Existing Features

### Restart the device if fails to connect the Wi-Fi at startup

Soon after configuring the WiFi if device fails to connect to the WiFi, after 15 retries restart the device and this restart is limited to a maximum of 3 times

### Fix for the ‘Device not configured’ issue.

Added CRC updation, when config data is updated from server which was causing the issue. Added retry to improve EEPROM read/writes.

### Blue LED 10 second stable state

When running test connectivity, if response from server is received, but if it is not a valid response, it was missing to indicate this state. Added BLUE LED stable ON for 10 second to denote this state.

### WiFi disconnects after sending data to server

Since Stable Wi-Fi connectivity introduced in the last release, is said to be introducing issues in WiFi connectivity for some customers, the change is reverted and WiFi connection is disabled after a server connectivity and connects back as and when required. Drawbacks of this scheme is

* + 1. It will cause slight data latency from device side as 10 second state machine will spend certain cycles for WiFi connectivity actions every time before sending data to cloud.
    2. For any router/AP which is limited the connectivity to certain number, when device tries to connect, if that number is reached, router may not allow the device to get connected and may report as data not available in the server.

# V- iCUBE 0x0102, iCON 0x0202

## Enhancements/Fixes to Existing Features

### **Chance for data latency/data loss due to the code loopholes are fixed**

### **Frequent connection/disconnection of Wi-Fi is avoided**

### **RED LED in 5 second blink when mains failure is detected, removed.**

### **SSID Name exposed by the device will have firmware version string at the end**

# V- iCUBE 0x0101, iCON 0x0201

## Enhancements/Fixes to Existing Features

### **Issue in using Configuration tool and mobile app is fixed**

### **‘Connectivity test’ issue is fixed**

## **Known issues**

### **When tested mobile application using a mobile phone Xiaomi MiA1 android version 9 , socket connection to the device is not happening when mobile data is ON.**

# **V- iCUBE 0x0100, iCON 0x0200**

## Enhancements/Fixes to Existing Features

### **First stable release**